**test\_EEPROM**

* Function to initialize the EEPROM: all bits to 0
* Function to initialize the EEPROM after factory: for tests only

**test\_RTC\_NVRAM**

* Function to initialize the NVRAM of the RTC module: all bits to 0